SECTION  09 54 34 
 SUSPENDED MODULAR CEILING MODULES - ARBORISA

PART 1 - GENERAL

1.1  
RELATED DOCUMENTS


Drawings and General Conditions of Contract, including General and Supplementary Conditions and Divisions-1 Specification sections apply to work of this section.


1.2
SUMMARY

A.
Section Includes:

1.
Suspended Acoustical Arborisa® Modular Ceiling Modules

2.
Cable hangers and fasteners

B.
Related Sections:

1. Division 23 (15) Sections - HVAC

2. Division 26 (16) Sections - Electrical
1.3
REFERENCES

A.
Test Methods:

1. ASTM C 423 Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method.

2. ASTM E 84 Standard Test Method for Surface Burning Characteristics of Building Materials.
1.4
QUALITY ASSURANCE

A. Single-Source Responsibility:  Provide modules and method of attachment by a single manufacturer.

B. Coordination of Work:  Coordinate ceiling work with installers of related work including, but not limited to building insulation, gypsum board, light fixtures, mechanical systems, electrical systems, and sprinklers.

1.5
DELIVERY, STORAGE, AND HANDLING

A. Store the Acoustical Arborisa® modular ceiling modules in an interior location and keep in cartons prior to installation to avoid damage.

B. Exercise care in moving and opening cartons to prevent damage to the module face.
C. Handle modules carefully to avoid damaging units in any way.
1.6   PROJECT CONDITIONS
   A.   Space Enclosure: 
 


1.   Arborisa® Acoustical Modules:  All wet work must be complete and dry prior to installation.  Installation shall be carried out where the temperature is between 40 degrees F and 90 degrees F.  These temperature conditions must be maintained throughout the life of the warranty.  .  
1.7
WARRANTY

A.
Acoustical Ceiling Modules:  Submit a written warranty executed by the manufacturer, agreeing to repair or replace modules that fail within the warranty period.  Failures include, but are not limited to:
1. Modules:  Manufacturing defects.

2. Attachment devices:  Rusting and manufacturing defects.                          

B.
Warranty Period:

1.
Modules: One (1) year from date of substantial completion.

2.
Attachment devices:  One (1) year from date of substantial completion.

C.   Warranty Language:

Manufacturer’s products are expressly warranted for a period of one (1) year from purchase to be free from defects in material and workmanship, when installed according to manufacturer’s published installation procedures. During the warranty period manufacturer will repair or at its option replace the products that are proven to be defective. Manufacturer is NOT responsible for any intentional or accidental abuse, misuse, or neglect incurred on the original warranted product, and shall as determined by manufacturer, void the warranty.
PART 2 - PRODUCTS

2.1
MANUFACTURER

A. Arktura, LLC – 966 Sandhill Ave. Carson, CA 90746 -

P. 310-532-1050 

info@arktura.com

2.2
MODULE UNITS

A.
Modules:
1.   Pattern: Aura, Axil, Denza, Nest (Choose One)
2.   Surface Texture: Smooth texture
3.   Composition: PET plastic (up to 60% recycled) + Metal brackets
4.   Color: Color to be confirmed by Architect (Wood or Color Group A)
5.   Module Size: As shown on drawings

2.3
ATTACHMENT SYSTEM
A. Installation Hardware:

1/32” stainless braided Wire, stainless connector plates, and Griplock tensioning hardware

PART 3 - EXECUTION

3.1
PREPARATION

A.
Field verify each wall area and establish layout of modules. Coordinate setting drawings, diagrams, templates, instructions, and directions for installation.  Module substructure shall be level and plumb. Module substructure shall be structurally sound as determined by that subcontractor’s engineer. Module substructure shall be free of defects detrimental to work and erected in accordance with established building tolerances.  
B.
Coordinate module layout with mechanical, electrical and sprinkler fixtures as required.
C.
Coordinate delivery of such items to project site.

3.2  INSTALLATION [by Others]

A.
Install modules in accordance with the manufacturer’s instructions and in compliance with the authorities having jurisdiction.
B.
Erect modules level and plumb, in proper alignment in relation to substructure framing and established lines.

C.
Module anchorage shall be structurally sound and per engineering recommendations.

D.
Locate and place wall modules level, plumb, and at indicated alignment with adjacent work. (Optional if vertical hung application)

E.   Do not locate the modules in the direct sunlight or sagging from heat and color fade may occur. 
3.3
ADJUSTING AND CLEANING

A.
Replace damaged and broken modules.
B. 
Routine maintenance of Arborisa® modules should consist of: Blot excess spills from material quickly. Wipe with a damp cloth. If stain persists, apply small quantities of carpet or upholstery shampoo solution with a damp cloth. Blot well with a clean cloth after each application of the solution. Warning, avoid excessive amounts of water. Note: Ensure adequate ventilation if the product is likely to be subject to excessive moisture

3.4  WASTE MANAGEMENT

A. Arborisa® may be disposed of in standard PET recycling stream provided that no disqualifying foreign matter has been affixed, such as adhesives. 

B. Waste Management:

a. Coordinate recycling of waste materials with Section [01 74 19 - Construction Waste Management and Disposal].

b. Collect recyclable waste and dispose of or recycle field generated construction waste created during demolition, construction or final cleaning.

c. Remove recycling containers and bins from site.
END OF SECTION
